--- trunk/tengDissertation/Methodology.tex	2006/06/11 03:11:06	2856
+++ trunk/tengDissertation/Methodology.tex	2006/06/16 01:53:48	2864
@@ -206,13 +206,9 @@ relaxation of the temperature to the target value.  To
 \end{equation}
 
 In eq.(\ref{eq:nosehooverext}), $\tau_T$ is the time constant for
-relaxation of the temperature to the target value.  To set values
-for $\tau_T$ or $T_{\mathrm{target}}$ in a simulation, one would use
-the {\tt tauThermostat} and {\tt targetTemperature} keywords in the
-{\tt .bass} file.  The units for {\tt tauThermostat} are fs, and the
-units for the {\tt targetTemperature} are degrees K.   The
-integration of the equations of motion is carried out in a
-velocity-Verlet style 2 part algorithm:
+relaxation of the temperature to the target value. The integration
+of the equations of motion is carried out in a velocity-Verlet style
+2 part algorithm:
 
 {\tt moveA:}
 \begin{align*}
